===================================README===================================
--------------------------FYP-20-S3-10 PROTOTYPE_01-------------------------
-----------------------------------KITESSH----------------------------------
---------------------------------VERSION 1.0--------------------------------
--------------------------------NOVEMBER 2020-------------------------------
============================================================================
****************************************************************************
============================================================================

================================PROJECT META================================

KiteSSH - An SSH, SFTP, SCP and P2P client for Windows

UNIVERSITY OF WOLLONGONG - CSIT321 [Project]

GROUP: FYP-20-S3-10 - EFFICIENT SSH TUNNELING

MEMBERS:

	Fratini Luca Project Manager lucafratini94@gmail.com
	Maurice Rizat Kasomwung Backend Programmer mauricerizat@gmail.com
	Lim Wei Zhi Maximillian Frontend Programmer azure.marine1@gmail.com
	Chua Man Fu UI/UX Designer manfularry35@gmail.com
	Pang Chun Weng Software Tester pangchunweng1993@gmail.com


SUPERVISOR: Japit Sionggo
ASSESSOR: Tian Sion Hui

VERSION: 1.0
DATE: November 2020

============================================================================

================================REQUIREMENTS================================

This KiteSSH Application is meant for Microsoft Windows operating systems.
Windows 10 is recommended.

Java Runtime Environment (Minimum Version 1.8.0) is required to run the 
application.

============================================================================

=================================DISCLAIMER=================================

For the P2P features of KiteSSH, certificate checks are bypassed. As such, 
it is essential to be aware of the connecting client when setting up a 
listening server with the application's P2P feature. Passwords are not 
required to set up a P2P server but it is highly recommended.

When setting up a P2P Server with KiteSSH, if the "host address" field is 
left blank, the application will attempt to automatically detect the 
machine's IP address. Manual address specification may, however, be require 
in the case of multiple network interfaces.

============================================================================